{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["Revision History","1. R528-S2 Pin Characteristics","2. R528-S2 GPIO Multiplexing","3. R528-S2 Signal Description","Declaration"],"not_rendered":{"external_links":1,"defined_names":16},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Revision History","index":0,"n_rows":3,"n_cols":4,"rows_kept":3,"merged":[[0,0,0,3]],"flags":["formulas_cached_only"]}
["Revision History"]
["Revision","Date","Author","Description"]
["1.0","October 18,2021","AWA1896","Initial release version."]

{"sheet":"1. R528-S2 Pin Characteristics","index":1,"n_rows":172,"n_cols":7,"rows_kept":172,"merged":[[1,0,1,6],[3,0,3,6],[17,0,17,6],[27,0,27,6],[53,0,53,6],[73,0,73,6],[82,0,82,6],[103,0,103,6],[105,0,105,6],[107,0,107,6],[110,0,110,6],[115,0,115,6],[120,0,120,6],[148,0,148,6],[153,0,153,6],[157,0,157,6],[159,0,159,6],[168,0,168,6],[171,0,192,6]],"flags":["formulas_cached_only"]}
["Ball#","Pin Name[2] ","Type","Ball Reset State","Pull Up/Down","Default Buffer Strength  (mA)","Power Supply"]
["SDRAM"]
["K11,K12,L12, M12,N12","VCC-DRAM","P","NA","NA","NA","NA"]
["GPIOB"]
["D16","PB0","I/O","Z","PU/PD",4,"VCC-IO"]
["D17","PB1","I/O","Z","PU/PD",4,"VCC-IO"]
["M16","PB2","I/O","Z","PU/PD",4,"VCC-IO"]
["M17","PB3","I/O","Z","PU/PD",4,"VCC-IO"]
["M18","PB4","I/O","Z","PU/PD",4,"VCC-IO"]
["L16","PB5","I/O","Z","PU/PD",4,"VCC-IO"]
["L17","PB6","I/O","Z","PU/PD",4,"VCC-IO"]
["K16","PB7","I/O","Z","PU/PD",4,"VCC-IO"]
["D18","PB8","I/O","Z","PU/PD",4,"VCC-IO"]
["C16","PB9","I/O","Z","PU/PD",4,"VCC-IO"]
["C18","PB10","I/O","Z","PU/PD",4,"VCC-IO"]
["C17","PB11","I/O","Z","PU/PD",4,"VCC-IO"]
["B18","PB12","I/O","Z","PU/PD",4,"VCC-IO"]
["GPIOC"]
["L3","PC0","I/O","Z","PU/PD",4,"VCC-PC"]
["L2","PC1","I/O","Z","PU/PD",4,"VCC-PC"]
["L1","PC2","I/O","Z","PU/PD",4,"VCC-PC"]
["M3","PC3","I/O","PU","PU/PD",4,"VCC-PC"]
["M2","PC4","I/O","PU","PU/PD",4,"VCC-PC"]
["N3","PC5","I/O","PU","PU/PD",4,"VCC-PC"]
["N2","PC6","I/O","Z","PU/PD",4,"VCC-PC"]
["N1","PC7","I/O","Z","PU/PD",4,"VCC-PC"]
["F5","VCC-PC","P","NA","NA","NA","NA"]
["GPIOD"]
["T12","PD0","I/O","Z","PU/PD",4,"VCC-PD"]
["U12","PD1","I/O","Z","PU/PD",4,"VCC-PD"]
["U13","PD2","I/O","Z","PU/PD",4,"VCC-PD"]
["V13","PD3","I/O","Z","PU/PD",4,"VCC-PD"]
["T14","PD4","I/O","Z","PU/PD",4,"VCC-PD"]
["U14","PD5","I/O","Z","PU/PD",4,"VCC-PD"]
["U15","PD6","I/O","Z","PU/PD",4,"VCC-PD"]
["V15","PD7","I/O","Z","PU/PD",4,"VCC-PD"]
["U16","PD8","I/O","Z","PU/PD",4,"VCC-PD"]
["V16","PD9","I/O","Z","PU/PD",4,"VCC-PD"]
["U17","PD10","I/O","Z","PU/PD",4,"VCC-PD"]
["U18","PD11","I/O","Z","PU/PD",4,"VCC-PD"]
["T17","PD12","I/O","Z","PU/PD",4,"VCC-PD"]
["T18","PD13","I/O","Z","PU/PD",4,"VCC-PD"]
["R16","PD14","I/O","Z","PU/PD",4,"VCC-PD"]
["R17","PD15","I/O","Z","PU/PD",4,"VCC-PD"]
["P17","PD16","I/O","Z","PU/PD",4,"VCC-PD"]
["P18","PD17","I/O","Z","PU/PD",4,"VCC-PD"]
["N16","PD18","I/O","Z","PU/PD",4,"VCC-PD"]
["N17","PD19","I/O","Z","PU/PD",4,"VCC-PD"]
["V11","PD20","I/O","Z","PU/PD",4,"VCC-PD"]
["U11","PD21","I/O","Z","PU/PD",4,"VCC-PD"]
["T11","PD22","I/O","Z","PU/PD",4,"VCC-PD"]
["K13","VCC-LVDS","P","NA","NA","NA","NA"]
["H13","VCC-PD","P","NA","NA","NA","NA"]
["GPIOE"]
["V9","PE0","I/O","Z","PU/PD",4,"VCC-PE"]
["U9","PE1","I/O","Z","PU/PD",4,"VCC-PE"]
["T9","PE2","I/O","Z","PU/PD",4,"VCC-PE"]
["T8","PE3","I/O","Z","PU/PD",4,"VCC-PE"]
["V7","PE4","I/O","Z","PU/PD",4,"VCC-PE"]
["U7","PE5","I/O","Z","PU/PD",4,"VCC-PE"]
["T7","PE6","I/O","Z","PU/PD",4,"VCC-PE"]
["U6","PE7","I/O","Z","PU/PD",4,"VCC-PE"]
["T6","PE8","I/O","Z","PU/PD",4,"VCC-PE"]
["V5","PE9","I/O","Z","PU/PD",4,"VCC-PE"]
["U5","PE10","I/O","Z","PU/PD",4,"VCC-PE"]
["T5","PE11","I/O","Z","PU/PD",4,"VCC-PE"]
["U4","PE12","I/O","Z","PU/PD",4,"VCC-PE"]
["T4","PE13","I/O","Z","PU/PD",4,"VCC-PE"]
["V3","PE14","I/O","Z","PU/PD",4,"VCC-PE"]
["U3","PE15","I/O","Z","PU/PD",4,"VCC-PE"]
["V2","PE16","I/O","Z","PU/PD",4,"VCC-PE"]
["U2","PE17","I/O","Z","PU/PD",4,"VCC-PE"]
["G6","VCC-PE","P","NA","NA","NA","NA"]
["GPIOF"]
["G1","PF0","I/O","Z","PU/PD",4,"VCC-PF"]
["H3","PF1","I/O","Z","PU/PD",4,"VCC-PF"]
["J3","PF2","I/O","Z","PU/PD",4,"VCC-PF"]
["J2","PF3","I/O","Z","PU/PD",4,"VCC-PF"]
["J1","PF4","I/O","Z","PU/PD",4,"VCC-PF"]
["K3","PF5","I/O","Z","PU/PD",4,"VCC-PF"]
["K2","PF6","I/O","Z","PU/PD",4,"VCC-PF"]
["E6","VCC-PF","P","NA","NA","NA","NA"]
["GPIOG"]
["A2","PG0","I/O","Z","PU/PD",4,"VCC-PG"]
["C4","PG1","I/O","Z","PU/PD",4,"VCC-PG"]
["A3","PG2","I/O","Z","PU/PD",4,"VCC-PG"]
["C3","PG3","I/O","Z","PU/PD",4,"VCC-PG"]
["B1","PG4","I/O","Z","PU/PD",4,"VCC-PG"]
["B2","PG5","I/O","Z","PU/PD",4,"VCC-PG"]
["E3","PG6","I/O","Z","PU/PD",4,"VCC-PG"]
["E2","PG7","I/O","Z","PU/PD",4,"VCC-PG"]
["E1","PG8","I/O","Z","PU/PD",4,"VCC-PG"]
["F3","PG9","I/O","Z","PU/PD",4,"VCC-PG"]
["F2","PG10","I/O","Z","PU/PD",4,"VCC-PG"]
["G3","PG11","I/O","Z","PU/PD",4,"VCC-PG"]
["C2","PG12","I/O","Z","PU/PD",4,"VCC-PG"]
["C1","PG13","I/O","Z","PU/PD",4,"VCC-PG"]
["D3","PG14","I/O","Z","PU/PD",4,"VCC-PG"]
["D2","PG15","I/O","Z","PU/PD",4,"VCC-PG"]
["G2","PG16","I/O","Z","PU/PD",4,"VCC-PG"]
["B4","PG17","I/O","Z","PU/PD",4,"VCC-PG"]
["A4","PG18","I/O","Z","PU/PD",4,"VCC-PG"]
["E5","VCC-PG","P","NA","NA","NA","NA"]
["System"]
["T3","RESET","I, OD","NA","NA","NA","VCC-RTC"]
["LRADC"]
["C9","LRADC","AI","NA","NA","NA","AVCC"]
["GPADC"]
["B9","GPADC0","AI","NA","NA","NA","AVCC"]
["C8","GPADC1","AI","NA","NA","NA","AVCC"]
["TPADC"]
["A8","TP-X1","AI","NA","NA","NA","AVCC"]
["B8","TP-X2","AI","NA","NA","NA","AVCC"]
["B7","TP-Y1","AI","NA","NA","NA","AVCC"]
["C7","TP-Y2","AI","NA","NA","NA","AVCC"]
["USB"]
["C5","USB0-DM","A I/O","NA","NA","NA","VCC-IO"]
["B5","USB0-DP","A I/O","NA","NA","NA","VCC-IO"]
["B6","USB1-DM","A I/O","NA","NA","NA","VCC-IO"]
["A6","USB1-DP","A I/O","NA","NA","NA","VCC-IO"]
["Audio Codec"]
["B13","MICIN1P","AI","NA","NA","NA","AVCC"]
["C13","MICIN1N","AI","NA","NA","NA","AVCC"]
["A14","MICIN2P","AI","NA","NA","NA","AVCC"]
["B14","MICIN2N","AI","NA","NA","NA","AVCC"]
["B15","MICIN3P","AI","NA","NA","NA","AVCC"]
["C15","MICIN3N","AI","NA","NA","NA","AVCC"]
["E15","FMINR","AI","NA","NA","NA","AVCC"]
["D15","FMINL","AI","NA","NA","NA","AVCC"]
["F15","LINEINR","AI","NA","NA","NA","AVCC"]
["G15","LINEINL","AI","NA","NA","NA","AVCC"]
["C11","LINEOUTLN","AO","NA","NA","NA","AVCC"]
["B11","LINEOUTLP","AO","NA","NA","NA","AVCC"]
["B12","LINEOUTRN","AO","NA","NA","NA","AVCC"]
["A12","LINEOUTRP","AO","NA","NA","NA","AVCC"]
["C10","HPOUTR","AO","NA","NA","NA","HPVCC"]
["A10","HPOUTL","AO","NA","NA","NA","HPVCC"]
["B10","HPOUTFB","AI","NA","NA","NA","HPVCC"]
["F13","HPVCC","P","NA","NA","NA"," NA"]
["G12","HP-DET","AI","NA","NA","NA"," AVCC"]
["A16","HPLDOIN","P","NA","NA","NA"," VCC-IO"]
["E12","HBIAS","AO","NA","NA","NA","VCC-IO"]
["C12","MBIAS","AO","NA","NA","NA","VCC-IO"]
["F12","MIC-DET","AI","NA","NA","NA","AVCC"]
["B16","VRA1","AO","NA","NA","NA","AVCC"]
["B17","VRA2","AO","NA","NA","NA","AVCC"]
["E13","AVCC","P","NA","NA","NA","NA"]
["A17","AGND","G","NA","NA","NA","NA"]
["RTC & PLL"]
["T1","X32KIN","AI","NA","NA","NA","VCC-RTC"]
["T2","X32KOUT","AO","NA","NA","NA","VCC-RTC"]
["G5","VCC-RTC","P","NA","NA","NA","NA"]
["H5","VCC-PLL","P","NA","NA","NA","NA"]
["DCXO"]
["R1","DXIN","AI","NA","NA","NA","VCC-PLL"]
["R2","DXOUT","AO","NA","NA","NA","VCC-PLL"]
["P2","REFCLK-OUT","AO","NA","NA","NA","VCC-PLL"]
["NC"]
["J16, J17, K18, K17, G16, G17, F17, F18, E16, E17, H17, H18 , N11","NC","NA","NA","NA","NA","NA"]
["Power"]
["L5","LDO-IN","P","NA","NA","NA","NA"]
["J5","LDOA-OUT","P","NA","NA","NA","NA"]
["K5","LDOB-OUT","P","NA","NA","NA","NA"]
["G13","VCC-IO","P","NA","NA","NA","NA"]
["E10,E11,F10, F11","VDD-SYS","P","NA","NA","NA","NA"]
["E7,E8,F7,F8","VDD-CPU","P","NA","NA","NA","NA"]
["E9","VDD-CPUFB","P","NA","NA","NA","NA"]
["J13","VCC-1V8","P","NA","NA","NA","NA"]
["GND"]
["A1,A18,B3,C14,C6,F16,F9,G11,G7,G8,G9,H11,H12,H16,H2, H6,H7,H8,J12, J6,J7,J8,J9,L10,L13,L6,L8,L9, M10,M11,M13,M5,M6,M8, M9,N10,N13, N5,N7,N8,N9, P16,P3,R3,T10,T13,T15,T16, U1,U10,U8,V1,V17,V18","GND","G","NA","NA","NA","NA"]
[]
["Note:\n[1].Ball#: Package ball numbers associated with each signal.\n[2].Pin Name: The name of the package pin.\n[3].Type: Denotes the signal direction\n      I (Input), \n     O (Output), \n     I/O (Input/Output), \n     OD (Open-Drain),\n    A (Analog),\n    AI (Analog Input),\n    AO (Analog Output), \n    P (Power), \n    G (Ground)\n[4].Ball Reset State: The state of the terminal at reset. PU: pull up; PD: pull down; Z: high impedance.\n[5].Pull Up/Down: Denotes the presence of an internal pull-up or pull-down resistor. Pull-up and pull-down resistors can be enabled or disabled via software.\n[6].Default Buffer Strength: Defines the default drive strength of the associated output buffer. The maximum drive strength of each GPIO is 6 mA.\n[7].Power Supply: The voltage supply for the IO buffers of the terminal.\n"]

{"sheet":"2. R528-S2 GPIO Multiplexing","index":2,"n_rows":99,"n_cols":12,"rows_kept":99,"merged":[[1,0,2,0],[1,1,2,1],[1,2,22,2],[1,3,2,3],[1,4,2,4],[1,5,2,5],[1,6,2,6],[1,8,2,8],[1,9,2,9],[1,10,2,10],[1,11,2,11],[10,0,12,0],[10,1,12,1],[10,3,12,3],[10,4,12,4],[10,5,12,5],[10,6,12,6],[10,8,12,8],[10,9,12,9],[10,10,12,10],[10,11,12,11],[13,0,16,0],[13,1,16,1],[13,3,16,3],[13,4,16,4],[13,5,16,5],[13,6,16,6],[13,8,16,8],[13,9,16,9],[13,10,16,10],[13,11,16,11],[17,0,18,0],[17,1,18,1],[17,3,18,3],[17,4,18,4],[17,5,18,5],[17,6,18,6],[17,8,18,8],[17,9,18,9],[17,10,18,10],[17,11,18,11],[19,0,20,0],[19,1,20,1],[19,3,20,3],[19,4,20,4],[19,5,20,5],[19,6,20,6],[19,8,20,8],[19,9,20,9],[19,10,20,10],[19,11,20,11],[21,0,22,0],[21,1,22,1],[21,3,22,3],[21,4,22,4],[21,5,22,5],[21,6,22,6],[21,8,22,8],[21,9,22,9],[21,10,22,10],[21,11,22,11],[23,2,30,2],[31,2,53,2],[54,2,72,2],[55,0,56,0],[55,1,56,1],[55,3,56,3],[55,4,56,4],[55,5,56,5],[55,6,56,6],[55,7,56,7],[55,8,56,8],[55,9,56,9],[55,11,56,11],[73,2,79,2],[80,2,98,2]],"flags":["formulas_cached_only"]}
["Ball","Pin Name","GPIO Group","IO Type","Function2","Function3","Function4","Function5","Function6","Function7","Function8","Function14"]
["D16","PB0","GPIOB","I/O","PWM3","IR-TX","TWI2-SCK","SPI1-WP/","UART0-TX","UART2-TX","OWA-OUT","PB-EINT0"]
[{"$nulls":7},"DBI-TE"]
["D17","PB1",null,"I/O","PWM4","I2S2-DOUT3","TWI2-SDA","I2S2-DIN3","UART0-RX","UART2-RX","IR-RX","PB-EINT1"]
["M16","PB2",null,"I/O","LCD0-D0","I2S2-DOUT2","TWI0-SDA","I2S2-DIN2","LCD0-D18","UART4-TX",null,"PB-EINT2"]
["M17","PB3",null,"I/O","LCD0-D1","I2S2-DOUT1","TWI0-SCK","I2S2-DIN0","LCD0-D19","UART4-RX",null,"PB-EINT3"]
["M18","PB4",null,"I/O","LCD0-D8","I2S2-DOUT0","TWI1-SCK","I2S2-DIN1","LCD0-D20","UART5-TX",null,"PB-EINT4"]
["L16","PB5",null,"I/O","LCD0-D9","I2S2-BCLK","TWI1-SDA","PWM0","LCD0-D21","UART5-RX",null,"PB-EINT5"]
["L17","PB6",null,"I/O","LCD0-D16","I2S2-LRCK","TWI3-SCK","PWM1","LCD0-D22","UART3-TX","CPUBIST0","PB-EINT6"]
["K16","PB7",null,"I/O","LCD0-D17","I2S2-MCLK","TWI3-SDA","IR-RX","LCD0-D23","UART3-RX","CPUBIST1","PB-EINT7"]
["D18","PB8",null,"I/O","DMIC-DATA3","PWM5","TWI2-SCK","SPI1-HOLD/","UART0-TX","UART1-TX",null,"PB-EINT8"]
[{"$nulls":7},"DBI-DCX/"]
[{"$nulls":7},"DBI-WRX"]
["C16","PB9",null,"I/O","DMIC-DATA2","PWM6","TWI2-SDA","SPI1-MISO/","UART0-RX","UART1-RX",null,"PB-EINT9"]
[{"$nulls":7},"DBI-SDI/"]
[{"$nulls":7},"DBI-TE/"]
[{"$nulls":7},"DBI-DCX"]
["C18","PB10",null,"I/O","DMIC-DATA1","PWM7","TWI0-SCK","SPI1-MOSI/","CLK-FANOUT0","UART1-RTS",null,"PB-EINT10"]
[{"$nulls":7},"DBI-SDO"]
["C17","PB11",null,"I/O","DMIC-DATA0","PWM2","TWI0-SDA","SPI1-CLK/","CLK-FANOUT1","UART1-CTS",null,"PB-EINT11"]
[{"$nulls":7},"DBI-SCLK"]
["B18","PB12",null,"I/O","DMIC-CLK","PWM0","OWA-IN","SPI1-CS/","CLK-FANOUT2","IR-RX",null,"PB-EINT12"]
[{"$nulls":7},"DBI-CSX"]
["L3","PC0","GPIOC","I/O","UART2-TX","TWI2-SCK","LEDC-DO",{"$nulls":4},"PC-EINT0"]
["L2","PC1",null,"I/O","UART2-RX","TWI2-SDA",{"$nulls":5},"PC-EINT1"]
["L1","PC2",null,"I/O","SPI0-CLK","SDC2-CLK",{"$nulls":5},"PC-EINT2"]
["M3","PC3",null,"I/O","SPI0-CS0","SDC2-CMD",{"$nulls":5},"PC-EINT3"]
["M2","PC4",null,"I/O","SPI0-MOSI","SDC2-D2","BOOT-SEL0",{"$nulls":4},"PC-EINT4"]
["N3","PC5",null,"I/O","SPI0-MISO","SDC2-D1","BOOT-SEL1",{"$nulls":4},"PC-EINT5"]
["N2","PC6",null,"I/O","SPI0-WP","SDC2-D0","UART3-TX","TWI3-SCK","DBG-CLK",null,null,"PC-EINT6"]
["N1","PC7",null,"I/O","SPI0-HOLD","SDC2-D3","UART3-RX","TWI3-SDA","TCON-TRIG",null,null,"PC-EINT7"]
["T12","PD0","GPIOD","I/O","LCD0-D2","LVDS0-V0P","DSI-D0P","TWI0-SCK",{"$nulls":3},"PD-EINT0"]
["U12","PD1",null,"I/O","LCD0-D3","LVDS0-V0N","DSI-D0N","UART2-TX",{"$nulls":3},"PD-EINT1"]
["U13","PD2",null,"I/O","LCD0-D4","LVDS0-V1P","DSI-D1P","UART2-RX",{"$nulls":3},"PD-EINT2"]
["V13","PD3",null,"I/O","LCD0-D5","LVDS0-V1N","DSI-D1N","UART2-RTS",{"$nulls":3},"PD-EINT3"]
["T14","PD4",null,"I/O","LCD0-D6","LVDS0-V2P","DSI-CKP","UART2-CTS",{"$nulls":3},"PD-EINT4"]
["U14","PD5",null,"I/O","LCD0-D7","LVDS0-V2N","DSI-CKN","UART5-TX",{"$nulls":3},"PD-EINT5"]
["U15","PD6",null,"I/O","LCD0-D10","LVDS0-CKP","DSI-D2P","UART5-RX",{"$nulls":3},"PD-EINT6"]
["V15","PD7",null,"I/O","LCD0-D11","LVDS0-CKN","DSI-D2N","UART4-TX",{"$nulls":3},"PD-EINT7"]
["U16","PD8",null,"I/O","LCD0-D12","LVDS0-V3P","DSI-D3P","UART4-RX",{"$nulls":3},"PD-EINT8"]
["V16","PD9",null,"I/O","LCD0-D13","LVDS0-V3N","DSI-D3N","PWM6",{"$nulls":3},"PD-EINT9"]
["U17","PD10",null,"I/O","LCD0-D14","LVDS1-V0P","SPI1-CS/DBI-CSX","UART3-TX",{"$nulls":3},"PD-EINT10"]
["U18","PD11",null,"I/O","LCD0-D15","LVDS1-V0N","SPI1-CLK/DBI-SCLK","UART3-RX",{"$nulls":3},"PD-EINT11"]
["T17","PD12",null,"I/O","LCD0-D18","LVDS1-V1P","SPI1-MOSI/DBI-SDO","TWI0-SDA",{"$nulls":3},"PD-EINT12"]
["T18","PD13",null,"I/O","LCD0-D19","LVDS1-V1N","SPI1-MISO/DBI-SDI/DBI-TE/DBI-DCX","UART3-RTS",{"$nulls":3},"PD-EINT13"]
["R16","PD14",null,"I/O","LCD0-D20","LVDS1-V2P","SPI1-HOLD/DBI-DCX/DBI-WRX","UART3-CTS",{"$nulls":3},"PD-EINT14"]
["R17","PD15",null,"I/O","LCD0-D21","LVDS1-V2N","SPI1-WP/DBI-TE","IR-RX",{"$nulls":3},"PD-EINT15"]
["P17","PD16",null,"I/O","LCD0-D22","LVDS1-CKP","DMIC-DATA3","PWM0",{"$nulls":3},"PD-EINT16"]
["P18","PD17",null,"I/O","LCD0-D23","LVDS1-CKN","DMIC-DATA2","PWM1",{"$nulls":3},"PD-EINT17"]
["N16","PD18",null,"I/O","LCD0-CLK","LVDS1-V3P","DMIC-DATA1","PWM2",{"$nulls":3},"PD-EINT18"]
["N17","PD19",null,"I/O","LCD0-DE","LVDS1-V3N","DMIC-DATA0","PWM3",{"$nulls":3},"PD-EINT19"]
["V11","PD20",null,"I/O","LCD0-HSYNC","TWI2-SCK","DMIC-CLK","PWM4",{"$nulls":3},"PD-EINT20"]
["U11","PD21",null,"I/O","LCD0-VSYNC","TWI2-SDA","UART1-TX","PWM5",{"$nulls":3},"PD-EINT21"]
["T11","PD22",null,"I/O","OWA-OUT","IR-RX","UART1-RX","PWM7",{"$nulls":3},"PD-EINT22"]
["V9","PE0","GPIOE","I/O","NCSI0-HSYNC","UART2-RTS","TWI1-SCK","LCD0-HSYNC",null,null,"RGMII-RXCTRL/RMII-CRS-DV","PE-EINT0"]
["U9","PE1",null,"I/O","NCSI0-VSYNC","UART2-CTS","TWI1-SDA","LCD0-VSYNC",null,null,"RGMII-RXD0/","PE-EINT1"]
["U9",{"$nulls":9},"RMII-RXD0"]
["T9","PE2",null,"I/O","NCSI0-PCLK","UART2-TX","TWI0-SCK","CLK-FANOUT0","UART0-TX",null,"RGMII-RXD1/ RMII-RXD1","PE-EINT2"]
["T8","PE3",null,"I/O","NCSI0-MCLK","UART2-RX","TWI0-SDA","CLK-FANOUT1","UART0-RX",null,"RGMII-TXCK/ RMII-TXCK","PE-EINT3"]
["V7","PE4",null,"I/O","NCSI0-D0","UART4-TX","TWI2-SCK","CLK-FANOUT2","D-JTAG-MS",null,"RGMII-TXD0/ RMII-TXD0","PE-EINT4"]
["U7","PE5",null,"I/O","NCSI0-D1","UART4-RX","TWI2-SDA","LEDC-DO","D-JTAG-DI",null,"RGMII-TXD1/ RMII-TXD1","PE-EINT5"]
["T7","PE6",null,"I/O","NCSI0-D2","UART5-TX","TWI3-SCK","OWA-IN","D-JTAG-DO",null,"RGMII-TXCTRL/RMII-TXEN","PE-EINT6"]
["U6","PE7",null,"I/O","NCSI0-D3","UART5-RX","TWI3-SDA","OWA-OUT","D-JTAG-CK",null,"RGMII-CLKIN/RMII-RXER","PE-EINT7"]
["T6","PE8",null,"I/O","NCSI0-D4","UART1-RTS","PWM2","UART3-TX","JTAG-MS",null,"MDC","PE-EINT8"]
["V5","PE9",null,"I/O","NCSI0-D5","UART1-CTS","PWM3","UART3-RX","JTAG-DI",null,"MDIO","PE-EINT9"]
["U5","PE10",null,"I/O","NCSI0-D6","UART1-TX","PWM4","IR-RX","JTAG-DO",null,"EPHY-25M","PE-EINT10"]
["T5","PE11",null,"I/O","NCSI0-D7","UART1-RX","I2S0-DOUT3","I2S0-DIN3","JTAG-CK",null,"RGMII-TXD2","PE-EINT11"]
["U4","PE12",null,"I/O","TWI2-SCK","NCSI0-FIELD","I2S0-DOUT2","I2S0-DIN2",null,null,"RGMII-TXD3","PE-EINT12"]
["T4","PE13",null,"I/O","TWI2-SDA","PWM5","I2S0-DOUT0","I2S0-DIN1","DMIC-DATA3",null,"RGMII-RXD2","PE-EINT13"]
["V3","PE14",null,"I/O","TWI1-SCK","D-JTAG-MS","I2S0-DOUT1","I2S0-DIN0","DMIC-DATA2",null,"RGMII-RXD3","PE-EINT14"]
["U3","PE15",null,"I/O","TWI1-SDA","D-JTAG-DI","PWM6","I2S0-LRCK","DMIC-DATA1",null,"RGMII-RXCK","PE-EINT15"]
["V2","PE16",null,"I/O","TWI3-SCK","D-JTAG-DO","PWM7","I2S0-BCLK","DMIC-DATA0",null,null,"PE-EINT16"]
["U2","PE17",null,"I/O","TWI3-SDA","D-JTAG-CK","IR-TX","I2S0-MCLK","DMIC-CLK",null,null,"PE-EINT17"]
["G1","PF0","GPIOF","I/O","SDC0-D1","JTAG-MS",null,"I2S2-DOUT1","I2S2-DIN0",null,null,"PF-EINT0"]
["H3","PF1",null,"I/O","SDC0-D0","JTAG-DI",null,"I2S2-DOUT0","I2S2-DIN1",null,null,"PF-EINT1"]
["J3","PF2",null,"I/O","SDC0-CLK","UART0-TX","TWI0-SCK","LEDC-DO","OWA-IN",null,null,"PF-EINT2"]
["J2","PF3",null,"I/O","SDC0-CMD","JTAG-DO",null,"I2S2-BCLK",{"$nulls":3},"PF-EINT3"]
["J1","PF4",null,"I/O","SDC0-D3","UART0-RX","TWI0-SDA","PWM6","IR-TX",null,null,"PF-EINT4"]
["K3","PF5",null,"I/O","SDC0-D2","JTAG-CK",null,"I2S2-LRCK",{"$nulls":3},"PF-EINT5"]
["K2","PF6",null,"I/O",null,"OWA-OUT","IR-RX","I2S2-MCLK","PWM5",null,null,"PF-EINT6"]
["A2","PG0","GPIOG","I/O","SDC1-CLK","UART3-TX","RGMII-RXCTRL/ RMII-CRS-DV","PWM7",{"$nulls":3},"PG-EINT0"]
["C4","PG1",null,"I/O","SDC1-CMD","UART3-RX","RGMII-RXD0/ RMII-RXD0","PWM6",{"$nulls":3},"PG-EINT1"]
["A3","PG2",null,"I/O","SDC1-D0","UART3-RTS","RGMII-RXD1/ RMII-RXD1","UART4-TX",{"$nulls":3},"PG-EINT2"]
["C3","PG3",null,"I/O","SDC1-D1","UART3-CTS","RGMII-TXCK/ RMII-TXCK","UART4-RX",{"$nulls":3},"PG-EINT3"]
["B1","PG4",null,"I/O","SDC1-D2","UART5-TX","RGMII-TXD0/ RMII-TXD0","PWM5",{"$nulls":3},"PG-EINT4"]
["B2","PG5",null,"I/O","SDC1-D3","UART5-RX","RGMII-TXD1/ RMII-TXD1","PWM4",{"$nulls":3},"PG-EINT5"]
["E3","PG6",null,"I/O","UART1-TX","TWI2-SCK","RGMII-TXD2","PWM1",{"$nulls":3},"PG-EINT6"]
["E2","PG7",null,"I/O","UART1-RX","TWI2-SDA","RGMII-TXD3","OWA-IN",{"$nulls":3},"PG-EINT7"]
["E1","PG8",null,"I/O","UART1-RTS","TWI1-SCK","RGMII-RXD2","UART3-TX",{"$nulls":3},"PG-EINT8"]
["F3","PG9",null,"I/O","UART1-CTS","TWI1-SDA","RGMII-RXD3","UART3-RX",{"$nulls":3},"PG-EINT9"]
["F2","PG10",null,"I/O","PWM3","TWI3-SCK","RGMII-RXCK","CLK-FANOUT0","IR-RX",null,null,"PG-EINT10"]
["G3","PG11",null,"I/O","I2S1-MCLK","TWI3-SDA","EPHY-25M","CLK-FANOUT1","TCON-TRIG",null,null,"PG-EINT11"]
["C2","PG12",null,"I/O","I2S1-LRCK","TWI0-SCK","RGMII-TXCTRL/ RMII-TXEN","CLK-FANOUT2","PWM0","UART1-TX",null,"PG-EINT12"]
["C1","PG13",null,"I/O","I2S1-BCLK","TWI0-SDA","RGMII-CLKIN/ RMII-RXER","PWM2","LEDC-DO","UART1-RX",null,"PG-EINT13"]
["D3","PG14",null,"I/O","I2S1-DIN0","TWI2-SCK","MDC","I2S1-DOUT1","SPI0-WP","UART1-RTS",null,"PG-EINT14"]
["D2","PG15",null,"I/O","I2S1-DOUT0","TWI2-SDA","MDIO","I2S1-DIN1","SPI0-HOLD","UART1-CTS",null,"PG-EINT15"]
["G2","PG16",null,"I/O","IR-RX","TCON-TRIG","PWM5","CLK-FANOUT2","OWA-IN","LEDC-DO",null,"PG-EINT16"]
["B4","PG17",null,"I/O","UART2-TX","TWI3-SCK","PWM7","CLK-FANOUT0","IR-TX","UART0-TX",null,"PG-EINT17"]
["A4","PG18",null,"I/O","UART2-RX","TWI3-SDA","PWM6","CLK-FANOUT1","OWA-OUT","UART0-RX",null,"PG-EINT18"]

{"sheet":"3. R528-S2 Signal Description","index":3,"n_rows":207,"n_cols":3,"rows_kept":207,"merged":[[1,0,1,2],[3,0,3,2],[6,0,6,2],[11,0,11,2],[15,0,15,2],[20,0,20,2],[23,0,23,2],[28,0,28,2],[30,0,30,2],[58,0,58,2],[65,0,65,2],[74,0,74,2],[79,0,79,2],[86,0,86,2],[96,0,96,2],[112,0,112,2],[115,0,115,2],[132,0,132,2],[135,0,135,2],[137,0,137,2],[144,0,144,2],[146,0,146,2],[148,0,148,2],[150,0,150,2],[170,0,170,2],[189,0,189,2],[198,0,198,2]],"flags":["formulas_cached_only"]}
["Signal Name","Description","Type"]
["DRAM"]
["VCC-DRAM","DRAM Power Supply","P"]
["System Control"]
["BOOT-SEL[1:0]","Boot Media Select","I"]
["RESET","Reset Signal (low active)","I, OD"]
["Clock"]
["X32KIN","Clock Input of 32.768 kHz Crystal","AI"]
["X32KOUT","Clock Output of 32.768 kHz Crystal","AO"]
["VCC-RTC","RTC Power","P"]
["VCC-PLL","PLL Power Supply","P"]
["DCXO"]
["REFCLK-OUT","Digital Compensated Crystal Oscillator Clock Fanout","AO"]
["DXIN","Digital Compensated Crystal Oscillator Input","AI"]
["DXOUT","Digital Compensated Crystal Oscillator Output","AO"]
["USB"]
["USB0-DM","USB DRD Data Signal DM","A I/O"]
["USB0-DP","USB DRD Data Signal DP","A I/O"]
["USB1-DM","USB HOST Data Signal DM","A I/O"]
["USB1-DP","USB HOST Data Signal DP","A I/O"]
["GPADC"]
["GPADC0","General Purpose ADC Input Channel 0","AI"]
["GPADC1","General Purpose ADC Input Channel 1","AI"]
["TPADC"]
["TP-X1","Touch Panel X1 Input","AI"]
["TP-X2","Touch Panel X2 Input","AI"]
["TP-Y1","Touch Panel Y1 Input","AI"]
["TP-Y2","Touch Panel Y2 Input","AI"]
["LRADC"]
["LRADC","Low Rate ADC","AI"]
["AUDIO CODEC"]
["LINEOUTLN","Lineout Left Channel Negative Differential Output","AO"]
["LINEOUTLP","Lineout Left Channel Positive Differential Output","AO"]
["LINEOUTRN","Lineout Right Channel Negative Differential Output","AO"]
["LINEOUTRP","Lineout Right Channel Positive Differential Output","AO"]
["HPOUTR","Headphone Right Output","AO"]
["HPOUTL","Headphone Light Output","AO"]
["HPOUTFB","Pseudo Differential Headphone Ground Reference","AI"]
["HPVCC","Headphone Power 1.8 V","P"]
["MICIN1P","Microphone Differential Positive Input 1","AI"]
["MICIN1N","Microphone Differential Negative Input 1","AI"]
["MICIN2P","Microphone Differential Positive Input 2","AI"]
["MICIN2N","Microphone Differential Negative Input 2","AI"]
["MICIN3P","Microphone Differential Positive Input 3","AI"]
["MICIN3N","Microphone Differential Negative Input 3","AI"]
["FMINR","FMIN Right Input","AI"]
["FMINL","FMIN Left Input","AI"]
["LINEINR","LINEIN Right Single-End Input ","AI"]
["LINEINL","LINEIN Left Single-End Input","AI"]
["HP-DET","Headphone Jack Detect","AI"]
["HPLDOIN","Headphone LDO","P"]
["HBIAS","Second Bias Voltage Output for Headset Microphone","AO"]
["MBIAS","First Bias Voltage Output for Main Microphone","AO"]
["MIC-DET","Headphone MIC Detect","AI"]
["VRA1","Internal Reference Voltage","AO"]
["VRA2","Internal Reference Voltage","AO"]
["AVCC","Power Supply for Analog Part","P"]
["AGND","Analog Ground","G"]
["LCD"]
["LCD0-D[23:0]","LCD Data Output","O"]
["LCD0-CLK","LCD Clock\nThe pixel data are synchronized by this clock","O"]
["LCD0-VSYNC","LCD Vertical Sync\nIt indicates one new frame","O"]
["LCD0-HSYNC","LCD Horizontal Sync\nIt indicates one new scan line","O"]
["LCD0-DE","LCD Data Output Enable","O"]
["TCON-TRIG","LCD Sync (TCON outputs to LCD for sync)","O"]
["LVDS"]
["LVDS0-CKP","LVDS0 Positive Port of Clock","O"]
["LVDS0-CKN","LVDS0 Negative Port of Clock","O"]
["LVDS0-V[3:0]P","LVDS0 Positive Port of Data Channel [3:0]","O"]
["LVDS0-V[3:0]N","LVDS0 Negative Port of Data Channel [3:0]","O"]
["LVDS1-CKP","LVDS1 Positive Port of Clock","O"]
["LVDS1-CKN","LVDS1 Negative Port of Clock","O"]
["LVDS1-V[3:0]P","LVDS1 Positive Port of Data Channel [3:0]","O"]
["LVDS1-V[3:0]N","LVDS1 Negative Port of Data Channel [3:0]","O"]
["DSI"]
["DSI-D[3:0]P","DSI Differential Data [3:0] Positive Signal","O"]
["DSI-D[3:0]N","DSI Differential Data [3:0] Negative Signal","O"]
["DSI-CKP","DSI Differential Clock Positive Signal","O"]
["DSI-CKN","DSI Differential Clock Negative Signal","O"]
["Parallel CSI"]
["NCSI0-PCLK","Parallel CSI Pixel Clock","I"]
["NCSI0-MCLK","Parallel CSI Master Clock","O"]
["NCSI0-HSYNC","Parallel CSI Horizontal Synchronous","I"]
["NCSI0-VSYNC","Parallel CSI Vertical Synchronous","I"]
["NCSI0-D[7:0]","Parallel CSI Data Bit","I"]
["NCSI0-FIELD","Parallel CSI Field Index","I"]
["SMHC"]
["SDC0-CMD","Command Signal for SD Card ","I/O, OD"]
["SDC0-CLK","Clock for SD Card ","O"]
["SDC0-D[3:0]","Data Input and Output for SD Card ","I/O"]
["SDC1-CMD","Command Signal for SDIO WIFI","I/O, OD"]
["SDC1-CLK","Clock for SDIO WIFI","O"]
["SDC1-D[3:0]","Data Input and Output for SDIO WIFI","I/O"]
["SDC2-CMD","Command Signal for eMMC","I/O, OD"]
["SDC2-CLK","Clock for eMMC","O"]
["SDC2-D[3:0]","Data Input and Output for eMMC","I/O"]
["I2S/PCM"]
["I2S0-MCLK","I2S0 Master Clock","O"]
["I2S0-LRCK","I2S0/PCM0 Sample Rate Clock/Sync","I/O"]
["I2S0-BCLK","I2S0/PCM0 Sample Rate Clock","I/O"]
["I2S0-DOUT[3:0]","I2S0/PCM0 Serial Data Output Channel [3:0]","O"]
["I2S0-DIN[3:0]","I2S0/PCM0 Serial Data Input Channel [3:0]","I"]
["I2S1-MCLK","I2S1 Master Clock","O"]
["I2S1-LRCK","I2S1/PCM1 Sample Rate Clock/Sync","I/O"]
["I2S1-BCLK","I2S1/PCM1 Sample Rate Clock","I/O"]
["I2S1-DOUT[1:0]","I2S1/PCM1 Serial Data Output Channel [1:0]","O"]
["I2S1-DIN[1:0]","I2S1/PCM1 Serial Data Input Channel [1:0]","I"]
["I2S2-MCLK","I2S2 Master Clock","O"]
["I2S2-LRCK","I2S2/PCM2 Sample Rate Clock/Sync","I/O"]
["I2S2-BCLK","I2S2/PCM2 Sample Rate Clock","I/O"]
["I2S2-DOUT[3:0]","I2S2/PCM2 Serial Data Output Channel [3:0]","O"]
["I2S2-DIN[3:0]","I2S2/PCM2 Serial Data Input Channel [3:0]","I"]
["DMIC"]
["DMIC-CLK","Digital Microphone Clock Output","O"]
["DMIC-DATA[3:0]","Digital Microphone Data Input","I"]
["EMAC"]
["RGMII-RXD3","RGMII Receive Data3 ","I"]
["RGMII-RXD2","RGMII Receive Data2","I"]
["RGMII-RXD1/RMII-RXD1","RGMII/RMII Receive Data1","I"]
["RGMII-RXD0/RMII-RXD0","RGMII/RMII Receive Data0","I"]
["RGMII-RXCK","RGMII Receive Clock","I"]
["RGMII-RXCTRL/RMII-CRS-DV","RGMII Receive Control/RMII Carrier Sense Receive Data Valid","I"]
["RGMII-CLKIN/RMII-RXER","RGMII Transmit Clock from External/RMII Receive Error","I"]
["RGMII-TXD3","RGMII Transmit Data3 ","O"]
["RGMII-TXD2","RGMII Transmit Data2","O"]
["RGMII-TXD1/RMII-TXD1","RGMII/RMII Transmit Data1","O"]
["RGMII-TXD0/RMII-TXD0","RGMII/RMII Transmit Data0","O"]
["RGMII-TXCK/RMII-TXCK","RGMII/RMII Transmit Clock\nFor RGMII, IO type is output;\nFor RMII, IO type is input","I/O"]
["RGMII-TXCTRL/RMII-TXEN","RGMII Transmit Control/RMII Transmit Enable","O"]
["MDC","RGMII/RMII Management Data Clock","O"]
["MDIO","RGMII/RMII Management Data Input/Output","I/O"]
["EPHY-25M","25 MHz Output for EMAC PHY","O"]
["OWA"]
["OWA-IN","One Wire Audio Input","I"]
["OWA-OUT","One Wire Audio Output","O"]
["LEDC"]
["LEDC-DO","Intelligent Control LED Signal Output","O"]
["Interrupt"]
["PB-EINT[12:0]","GPIO B Interrupt","I"]
["PC-EINT[7:0]","GPIO C Interrupt","I"]
["PD-EINT[22:0]","GPIO D Interrupt","I"]
["PE-EINT[17:0]","GPIO E Interrupt","I"]
["PF-EINT[6:0]","GPIO F Interrupt","I"]
["PG-EINT[18:0]","GPIO G Interrupt","I"]
["CIR Receiver"]
["IR-RX","Consumer Infrared Receiver ","I"]
["CIR Transmitter"]
["IR-TX","Consumer Infrared Transmitter","O"]
["PWM"]
["PWM[7:0]","Pulse Width Modulation Output Channel [7:0]","I/O"]
["SPI&SPI_DBI"]
["SPI0-CS","SPI0 Chip Select Signal, Low Active","I/O"]
["SPI0-CLK","SPI0 Clock Signal\nProvides serial interface timing.","I/O"]
["SPI0-MOSI","SPI0 Master Data Out, Slave Data In","I/O"]
["SPI0-MISO","SPI0 Master Data In, Slave Data Out","I/O"]
["SPI0-WP","SPI0 Write Protect, Low Active\nProtects the memory area against all program or erase instructions.\nIt also can be used for serial data input and output for SPI Quad Input or Quad Output mode.","I/O"]
["SPI0-HOLD","SPI0 Hold Signal\nPauses any serial communication with the device without deselecting or resetting it.\nIt also can be used for serial data input and output for SPI Quad Input or Quad Output mode. ","I/O"]
["SPI1-CS","SPI1 Chip Select Signal, Low Active","I/O"]
["SPI1-CLK","SPI1 Clock Signal\nProvides serial interface timing.","I/O"]
["SPI1-MOSI","SPI1 Master Data Out, Slave Data In","I/O"]
["SPI1-MISO","SPI1 Master Data In, Slave Data Out","I/O"]
["SPI1-WP","SPI1 Write Protect, Low Active\nProtects the memory area against all program or erase instructions.\nIt also can be used for serial data input and output for SPI Quad Input or Quad Output mode.","I/O"]
["SPI1-HOLD","SPI1 Hold Signal\nPauses any serial communication with the device without resetting it.\nIt also can be used for serial data input and output for SPI Quad Input or Quad Output mode.","I/O"]
["DBI-CSX","Chip Select Signal, Low Active","I/O"]
["DBI-SCLK","Serial Clock Signal ","I/O"]
["DBI-SDO","Data Output Signal","I/O"]
["DBI-SDI","Data Input Signal \nThe data is sampled on the rising edge and the falling edge","I/O"]
["DBI-TE","Tearing Effect Input \nIt is used to capture the external TE signal edge. The rising and falling edge is configurable.","I/O"]
["DBI-DCX","DCX pin is the select output signal of data and command.\nDCX = 0: register command;\nDCX = 1: data or parameter.","I/O"]
["DBI-WRX","When DBI operates in dual data lane format, the RGB666 format 2 can use WRX to transfer data","I/O"]
["UART "]
["UART0-TX","UART0 Data Transmit","O"]
["UART0-RX","UART0 Data Receive","I"]
["UART1-TX","UART1 Data Transmit","O"]
["UART1-RX","UART1 Data Receive","I"]
["UART1-CTS","UART1 Data Clear to Send","I"]
["UART1-RTS","UART1 Data Request to Send","O"]
["UART2-TX","UART2 Data Transmit","O"]
["UART2-RX","UART2 Data Receive","I"]
["UART2-CTS","UART2 Data Clear to Send","I"]
["UART2-RTS","UART2 Data Request to Send","O"]
["UART3-TX","UART3 Data Transmit","O"]
["UART3-RX","UART3 Data Receive","I"]
["UART3-CTS","UART3 Data Clear to Send","I"]
["UART3-RTS","UART3 Data Request to Send","O"]
["UART4-TX","UART4 Data Transmit","O"]
["UART4-RX","UART4 Data Receive","I"]
["UART5-TX","UART5 Data Transmit","O"]
["UART5-RX","UART5 Data Receive","I"]
["TWI"]
["TWI0-SCK","TWI0 Serial Clock Signal","I/O"]
["TWI0-SDA","TWI0 Serial Data Signal","I/O"]
["TWI1-SCK","TWI1 Serial Clock Signal","I/O"]
["TWI1-SDA","TWI1 Serial Data Signal","I/O"]
["TWI2-SCK","TWI2 Serial Clock Signal","I/O"]
["TWI2-SDA","TWI2 Serial Data Signal","I/O"]
["TWI3-SCK","TWI3 Serial Clock Signal","I/O"]
["TWI3-SDA","TWI3 Serial Data Signal","I/O"]
["JTAG"]
["D-JTAG-MS","DSP JTAG Mode Select","I"]
["D-JTAG-CK","DSP JTAG Clock Signal","I"]
["D-JTAG-DO","DSP JTAG Data Output","O"]
["D-JTAG-DI","DSP JTAG Data Input","I"]
["JTAG-MS","A7 JTAG Mode Select","I"]
["JTAG-CK","A7 JTAG Clock Signal","I"]
["JTAG-DO","A7 JTAG Data Output","O"]
["JTAG-DI","A7 JTAG Data Input","I"]

{"sheet":"Declaration","index":4,"n_rows":1,"n_cols":1,"rows_kept":1,"merged":[[0,0,34,7]],"flags":["formulas_cached_only"]}
["\nCopyright©2021 Allwinner Technology Co.,Ltd. All Rights Reserved.\nThis documentation is the original work and copyrighted property of Allwinner Technology Co.,Ltd (“Allwinner”). No part of this document may be reproduced, modify, publish or transmitted in any form or by any means without prior written consent of Allwinner.\n\nTrademarks and Permissions\nAllwinner and the Allwinner logo (incomplete enumeration) are trademarks of Allwinner Technology Co.,Ltd. All other trademarks, trade names, product or service names mentioned in this document are the property of their respective owners.\n\nImportant Notice and Disclaimer\nThe purchased products, services and features are stipulated by the contract made between Allwinner Technology Co.,Ltd (“Allwinner”) and the customer. All or part of the products, services and features described in this document may not be within the purchase scope or the usage scope. Please read the terms and conditions of the contract and relevant instructions carefully before using, and follow the instructions in this documentation strictly. Allwinner assumes no responsibility for the consequences of improper use (including but not limited to overvoltage, overclock, or excessive temperature).\nThe information in this document is provided just as a reference or typical applications, and is subject to change without notice. Every effort has been made in the preparation of this document to ensure accuracy of the contents. Allwinner is not responsible for any damage (including but not limited to indirect, incidental or special loss) or any infringement of third party rights arising from the use of this document. All statements, information, and recommendations in this document do not constitute a warranty or commitment of any kind, express or implied.\nNo license is granted by Allwinner herein express or implied or otherwise to any patent or intellectual property of Allwinner. Third party licences may be required to implement the solution/product. Customers shall be solely responsible to obtain all appropriately required third party licences. Allwinner shall not be liable for any licence fee or royalty due in respect of any required third party licence. Allwinner shall have no warranty, indemnity or other obligations with respect to third party licences. "]