{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Version History","A523 DRAM Support List"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Version History","index":0,"n_rows":17,"n_cols":7,"rows_kept":17,"flags":["formulas_cached_only"]}
{"$rows_empty":12}
[null,null,"Version","Date","Section/ Page","Author","Changes compared to previous issue"]
[null,null,"V1.0","2023-04-27",null,"LiJinbo","Initial version\n1.Add support list for A523\n2.update LPDDR4: H9HCNNNBKUMLXR-NEX、FLXC2004G-N1、KZDB42CAM-MD supported\n3.update LPDDR4X: H9HCNNNBKUMLXR-NEX supported"]
[null,null,"V1.1","2023-05-21",null,"LiJinbo","1.update LPDDR4: FLXC2004G-30、RS512M32LM4D2BDS-53BT、RS1G32LV4D2BDS-53BT、CXDB5CCBM-MJ-A、HG4XD04G-C2JA supported"]
[null,null,"V1.2","2023-06-02",null,"LiJinbo","1.update LPDDR4: CXDBBCCBM-MK-B、KALXX5S43AY2-T40"]
[null,null,"V1.3","2023-06-26",null,"LiJinbo","1.update LPDDR4: KALXX4S43AY2-T40、NT6AN512T32AV-J2、NT6AN1024F32AV-J2、GDB2D32MJ0-42M7、SM1G32Z32MD2DNQ-PG、SM1G32Z42MD2DNQ-PG A523 supported\n2.update LPDDR4: CXDB3ABAM-MK-A，DDR4: H5AN8G6NDJR、EM60E16NWBB "]

{"sheet":"A523 DRAM Support List","index":1,"n_rows":37,"n_cols":9,"rows_kept":37,"merged":[[0,0,0,10],[2,0,2,7],[3,0,3,7],[4,0,4,7],[5,0,5,7],[6,2,6,4],[6,7,6,9],[7,2,7,4],[7,7,7,9],[8,2,8,4],[8,6,9,6],[8,7,9,9],[9,2,9,4],[10,2,10,4],[10,6,11,6],[10,7,11,9],[11,2,11,4],[12,2,12,4],[15,0,16,0],[15,1,16,1],[15,2,16,2],[15,3,16,3],[15,4,16,4],[15,5,16,5],[15,6,15,8],[17,0,19,0],[20,0,21,0],[22,0,23,0],[24,0,26,0],[28,0,29,0],[30,0,31,0],[35,0,36,0]],"flags":["formulas_cached_only"]}
["Allwinnertech  A523 DRAM Support List"]
["General Description:"]
["1.The purpose of this document is the guide of DDR seclection for customer using our solution. "]
["2.There are some DDRs that not mentioned here. Since DDR is an universal device. So you can test it by yourself before mass production or send the sample to us for testing."]
["3. Since DDR is high speed device. Please directly copy AW PCB DRAM Part Template and follow our PCB Layout Guide."]
["Abbr. and Definition of Status:"]
[null,"Symbol","Definition",{"$nulls":3},"Abbr.","Definition"]
[null,"X","Do Not Support",{"$nulls":3},"STA","test status"]
[null,"D/S","Datasheet Support",{"$nulls":3},"freq","max frequency for MP. '/c' means compatible template"]
[null,"S/T","Sample Tested"]
[null,"√","Sample Tested and Mass Production",{"$nulls":3},"STD","verification standard\nC: commercial;  T: industrial"]
[]
[null,"NOTE","Part Number 标暗灰代表EOL"]
[]
[]
["Vendor","Part Number","Type","package","Density","Organization","A523"]
[{"$nulls":6},"STA","Freq","STD"]
["Hynix","H5AN8G6NDJR","DDR4","FBGA96","8Gb","512M×16"]
[null,"H9HCNNNBKUMLXR-NEX","LPDDR4","FBGA200","16Gb","512M×16×2CH","S/T",1200,"C"]
[null,"H9HCNNNBKUMLXR-NEX","LPDDR4X","FBGA200","16Gb","512M×16×2CH","S/T",1200,"C"]
["江波龙","FLXC2004G-N1","LPDDR4","FBGA200","32Gb","1G×16×2CH","S/T",1200,"C"]
[null,"FLXC2004G-30","LPDDR4","FBGA200","32Gb","1G×16×2CH","S/T",1200,"C"]
["晶存Rayson","RS512M32LM4D2BDS-53BT","LPDDR4","FBGA200","16Gb","512M×32","S/T",1200,"C"]
[null,"RS1G32LV4D2BDS-53BT","LPDDR4","FBGA200","32Gb","1G×32","S/T",1200,"C"]
["长鑫CXMT","CXDB5CCBM-MJ-A","LPDDR4","FBGA200","32Gb","512M×16×2CH×2CS","S/T",1200,"C"]
[null,"CXDBBCCBM-MK-B","LPDDR4","FBGA200","24Gb","384M×16×2CH×2CS","S/T",1200,"C"]
[null,"CXDB3ABAM-MK-A","LPDDR4","FBGA200","8Gb","256M×16×2CH"]
["宏芯宇","HG4XD04G-C2JA","LPDDR4","FBGA200","32Gb","512M×32×2CH","S/T",1200,"C"]
["康盈KOWIN","KALXX5S43AY2-T40","LPDDR4","FBGA200","32Gb","512M×16×2CH×2CS","S/T",1200,"C"]
[null,"KALXX4S43AY2-T40","LPDDR4","FBGA200","16Gb","256M×16×2CH×2CS","S/T",1200,"C"]
["南亚Nanya","NT6AN1024F32AV-J2","LPDDR4","FBGA200","32Gb","1G×16×2CH","S/T",1200,"C"]
[null,"NT6AN512T32AV-J2","LPDDR4","FBGA200","16Gb","512M×16×2CH","S/T",1200,"C"]
["Kazoom","KZDB42CAM-MD","LPDDR4","FBGA200","32Gb","512M×32×2CS","S/T",1200,"C"]
["晶凯","GDB2D32MJ0-42M7","LPDDR4","FBGA200","32Gb","1G×16×2CH","S/T",1200,"C"]
["钰创Etron","EM60E16NWBB","DDR4","FBGA96","4Gb","256M×16"]
["Micron","SM1G32Z32MD2DNQ-PG","LPDDR4","FBGA200","32Gb","1G×32","S/T",1200,"C"]
[null,"SM1G32Z42MD2DNQ-PG","LPDDR4","FBGA200","32Gb","1G×32","S/T",1200,"C"]