{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["1-封面","2-Note","3-补丁","4-器件列表","5-声明"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"1-封面","index":0,"n_rows":17,"n_cols":11,"rows_kept":17,"merged":[[16,9,16,11]],"flags":["formulas_cached_only"]}
{"$rows_empty":13}
[{"$nulls":10},"Allwinner Technology "]
[{"$nulls":10},"eMMC Support List"]
[{"$nulls":10},"V1.139"]
[{"$nulls":9},"2023-03-29"]

{"sheet":"2-Note","index":1,"n_rows":14,"n_cols":2,"rows_kept":14,"merged":[[1,0,1,1]],"flags":["formulas_cached_only"]}
[]
["• Note Introduction"]
[]
["Status","Description"]
["D/S","Datasheet Supported but Need Sample to Full Test"]
["S/T","Sample Full Test Passed and Supported"]
["√","Supported and Mass Production"]
["X","Not Supported"]
["(Blank)","Not Recommended or in Testing"]
["A3","Automotive AEC-Q100 Grade3"]
["A2","Automotive AEC-Q100 Grade2"]
["A1","Automotive AEC-Q100 Grade1"]
["I","Industrial Grade "]
["C","Commercial Grade"]

{"sheet":"3-补丁","index":2,"n_rows":42,"n_cols":4,"rows_kept":42,"merged":[[1,0,1,3],[4,3,4,16],[5,0,7,0],[5,3,5,16],[6,3,6,16],[7,3,7,16],[8,3,8,16],[9,0,10,0],[9,3,9,16],[10,3,10,16],[11,3,11,16],[12,3,12,16],[13,0,15,0],[13,1,15,1],[13,3,15,16],[16,0,17,0],[16,1,17,1],[16,3,16,16],[17,3,17,16],[18,0,19,0],[18,3,18,16],[19,3,19,16],[20,3,20,16],[21,0,23,0],[21,3,21,16],[22,3,22,16],[23,3,23,16],[24,3,24,16],[25,0,26,0],[25,3,25,16],[26,3,26,16],[27,3,27,16],[28,0,29,0],[28,3,28,16],[29,3,29,16],[30,0,31,0],[30,3,30,16],[31,3,31,16],[32,3,32,16],[33,0,34,0],[33,3,33,16],[34,3,34,16],[35,3,35,16],[36,3,36,16],[37,3,37,16],[38,3,38,16],[39,3,39,16],[40,3,40,16],[41,3,41,16]],"flags":["formulas_cached_only"]}
[]
["• Attention"]
[]
["This support list is based on the specified SD/eMMC driver version which includes sdk version and eMMC patch."]
["IC","SD/eMMC Version","SDK Version","eMMC_patch"]
["H3","V1.01","homlet4.4.2-h3-v1.0rc2 ","NO"]
[null,"V2.01","H3-linux4.4"]
[null,"V 3.01","H3-linux4.9"]
["R333","V1.01","R333-linux4.9","NO"]
["H8","V1.00","H8 V1.0","NO"]
[null,"v2.01","H8 linux4.4"]
["A83","V1.01","A83-android4.4.4-v0.9rc1","NO"]
["A80","V1.01","A80-v1.0-onda-rc3","NO"]
["A23","V1.10","A23-Android4.2-V2.0 ","A23_Android4.2_V2.0_Android4.4_V1.0&V2.0_emmc_patch_20140525"]
[null,null,"A23-Android4.4-V1.0 "]
[null,null,"A23-Android4.4-V2.0 "]
["A31(S)","V1.60","A31(S)-Android4.4","A31(S)_Android4.4_V4.4&V4.5&V4.6_nand2.0&emmc_patch_20140707.tar.gz"]
[null,null,"A31(S)-Android4.2","A31(S)_Android4.2_V3.0&V3.2&V3.3_nand2.0&emmc_patch_20140625.tar.gz"]
["A33","V1.01","A33-Android4.4.2-V1.0","NO"]
[null,"V2.01","A33-Android7.1.2","A33_Android7.1.2&emmc_patch_20170424&avoid_host_dat0_busy_state_isnot_consistent_with_cmd13_prg_state.patch"]
["A20","V1.60","A20-Homlet-Android4.2.2-SDK V2.1rc3","A20_homlet-sugar42-v2.1_update_mmc_driver_2015-10-10.rar"]
["A64","V1.01","exdroid-6.0.1_r3-a64-v2.0rc2\n","NO"]
[null,"V2.01","A64-linux4.4","NO"]
[null,"V3.01","A64-linux4.9","NO"]
["G102/G202","V1.01",null,"NO"]
["V40/A20E","V1.01",null,"NO"]
[null,"V2.01","T3-linux4.9","NO"]
["H5","V1.01",null,"NO"]
["H6","V1.01",null,"NO"]
[null,"V2.01","H6-linux4.9","NO"]
["A63","V1.01",null,"NO"]
[null,"V2.01","A63-linux4.9","NO"]
["V5","V1.01",null,"NO"]
["T7","V1.01",null,"NO"]
[null,"V2.01","linux4.9","NO"]
["A50","V1.01","A50-linux4.9","NO"]
["C600","V1.01","c600-linux3.10","NO"]
["V316","V1.01","v316-linux4.9","NO"]
["H616","V1.01","H616-linux4.9；H616-Uboot2018","NO"]
["T507","V1.01","T507-linux4.9；T507-Uboot2018","NO"]
["A100","V1.01","A100-linux4.9；A100-Uboot2018","NO"]
["R329","V1.01","R329-linux4.9；R329-Uboot2018","NO"]

{"sheet":"4-器件列表","index":3,"n_rows":306,"n_cols":10,"rows_kept":306,"merged":[[1,0,1,9],[3,0,5,0],[3,1,5,1],[3,2,5,2],[3,3,5,3],[3,4,5,4],[3,5,5,5],[3,6,5,6],[3,7,5,7],[3,9,5,9],[6,0,39,0],[40,0,81,0],[82,0,92,0],[93,0,122,0],[123,0,129,0],[130,0,155,0],[156,0,176,0],[177,0,210,0],[211,0,212,0],[214,0,217,0],[218,0,223,0],[224,0,229,0],[230,0,231,0],[232,0,235,0],[236,0,238,0],[239,0,242,0],[244,0,246,0],[247,0,248,0],[250,0,255,0],[257,0,258,0],[259,0,260,0],[261,0,272,0],[280,0,281,0],[282,0,285,0],[287,0,288,0],[289,0,290,0],[292,0,295,0],[296,0,297,0],[298,0,299,0],[300,0,301,0],[302,0,303,0]],"flags":["formulas_cached_only"]}
[]
["• Support List"]
[]
["Vendor","Capacity\n(B)","Part Number","eMMC\n/SD","Cell&Process","Pkg Size\n(mm)","Grade","Operating Temperature\n(Deg.C)","A523","Remark"]
[{"$nulls":8},"V1.01"]
[{"$nulls":8},"linux\n5.15"]
["Samsung","8G","KLM8G1WE4A-A001","v4.41",null,"12*16-BGA169",{"$nulls":3},"EOL"]
[null,"16G","KLMAG2WE4A-A001","v4.41",null,"12*16-BGA169",{"$nulls":3},"EOL"]
[null,"4G","KLM4G1FE3B-B001","v4.41",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"4G","KLM4G1YEMD-B031","v5.0","TLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","KLM8G1WEMB-B031","v5.0","TLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","KLMAG2WEMB-B031","v5.0","TLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"32G","KLMBG4WEBC-B031","v5.0","TLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","KLMAG2GEAC-B031","v5.0","MLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","KLM8G1GEAC-B031","v5.0","MLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"4G","KLM4G1FEAC-B031","v5.0","MLC/19nm","11*10-BGA153",{"$nulls":3},"EOL"]
[null,"32G","KLMBG4GEAC-B031","v5.0","MLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"32G","KLMBG4GE2A-A001","V4.5","MLC","12*16-BGA169",{"$nulls":3},"EOL"]
[null,"16G","KLMAG2GEND-B031","v5.0","MLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"32G","KLMBG4GEND-B031","v5.0","MLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"8G","KLM8G1WEPD-B031","v5.0","TLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"16G","KLMAG2WEPD-B031","v5.0","TLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"32G","KLMBG4WEBD-B031","v5.0","TLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"64G","KLMCG8GEND-B031","v5.0","MLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"8G","KLM8G1GEND-B031","v5.0","MLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"64G","KLMCG8WEBD-B031","v5.0","TLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"4G","KLM4G1FEPD-B031","v5.0","MLC/16nm","11*10-BGA153",null,"-25~+85","S/T"]
[null,"8G","KLM8G1GEME-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"16G","KLMAG1JENB-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"32G","KLMBG2JENB-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"64G","KLMCG4JENB-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"8G","KLM8G1GETF-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"16G","KLMAG1JETD-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"32G","KLMBG2JETD-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"64G","KLMCG4JETD-B041","v5.1","MLC/14nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"8G","KLM8G1GESD-B04P","v5.1","MLC/16nm","11.5*13-BGA153","A3","-40 ~ +85","S/T"]
[null,"16G","KLMAG2GESD-B04P","v5.1","MLC/16nm","11.5*13-BGA153","A3","-40 ~ +85"]
[null,"8G","KLM8G1GEUF-B04P","v5.1",null,"11.5*13-BGA153","A3","-40 ~ +85","S/T"]
[null,"16G","KLMAG2GEUF-B04P","v5.1",null,"11.5*13-BGA153","A3","-40 ~ +85","S/T"]
[null,"64G","KLMCG2UCTB-B041","v5.1",null,"11.5*13-BGA153",null,"-40 ~ +85"]
["Sandisk","8G","SDIN7DP2-8G","v4.5",null,"11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"16G","SDIN7DU2-16G","v4.41",null,"11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"4G","SDIN7DP2-4G","v4.5",null,"11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"8G","SDIN8DE1-8G","v4.5","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"8G","SDIN8DE2-8G","v4.5","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"8G","SDIN8DR1-8G","v4.51","TLC/1Ynm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","SDIN8DR1-16G","v4.51","TLC/1Ynm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"4G","SDIN8DE2-4G","v4.51","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"8G","SDIN7DU2-8G","v4.41",null,"11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"16G","SDIN7DP4-16G","V4.51","MLC","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"16G","SDIN8DE4-16G","v4.51","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"16G","SDIN8DE2-16G","v4.51","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"32G","SDIN8DE4-32G","v4.51","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"16G","SDIN9DW4-16G","v5.0","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"32G","SDIN9DW4-32G","v5.0","MLC/19nm","11.5*13-BGA153",null,"-25~+85",null,"EOL"]
[null,"64G","SDIN9DW4-64G","v5.1","MLC/20nm","11.5*13-BGA154",null,"-25~+85",null,"EOL"]
[null,"32G","SDIN9DS2-32G","v5.0","TLC/1Ynm","11.5*13-BGA153",null,"-25~+85",null,"IO电压不支持3.3V,EOL"]
[null,"16G","SDIN9DS2-16G","v5.0","TLC/1Ynm","11.5*13-BGA153",null,"-25~+85",null,"IO电压不支持3.3V,EOL"]
[null,"32G","SDINADF4-32G-L","v5.1","TLC/1Ynm","11.5*13-BGA153",{"$nulls":3},"IO电压不支持3.3V"]
[null,"8G","SDIN9DS2-8G","v5.0","TLC/1Ynm","11.5*13-BGA153",null,"-25~+85",null,"IO电压不支持3.3V,EOL"]
[null,"32G","SDINADF4-32G-H","v5.1","TLC/15nm","11.5*13-BGA153",null,"-25~+85",null,"IO电压不支持3.3V"]
[null,"16G","SDINADF4-16G-H","v5.1","TLC/15nm","11.5*13-BGA153",null,"-25~+85",null,"IO电压不支持3.3V"]
[null,"8G","SDIN8DE1-8G-XI","v4.51","MLC/1xnm","11.5*13-BGA153","I","-40 ~ +85",null,"EOL"]
[null,"8G","SDIN8DE2-8G-XA","v4.51","MLC/1xnm","11.5*13-BGA153","A3","-40 ~ +85",null,"EOL"]
[null,"8G","SDIN8DE1-8G-I","v4.51","MLC/1xnm","11.5*13-BGA153","I","-40 ~ +85",null,"EOL"]
[null,"8G","SDIN8DE2-8G-A","v4.51","MLC/1xnm","11.5*13-BGA153","A3","-40 ~ +85",null,"EOL"]
[null,"8G","SDINBDG4-8G","v5.1","MLC/1znm","11.5*13-BGA153",null,null,"S/T"]
[null,"8G","SDINBDG4-8G-B","v5.1","MLC/1znm","11.5*13-BGA153"]
[null,"16G","SDINBDG4-16G","v5.1","MLC/1znm","11.5*13-BGA153"]
[null,"32G","SDINBDG4-32G","v5.1","MLC/1znm","11.5*13-BGA153",null,null,"S/T"]
[null,"64G","SDINBDG4-64G","v5.1","MLC/1znm","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","SDINBDG4-16G-H","v5.1","MLC/1znm","11.5*13-BGA153"]
[null,"32G","SDINBDG4-32G-H","v5.1","MLC/1znm","11.5*13-BGA153",null,null,"S/T"]
[null,"32G","SDINBDA4-32G","v5.1","3D TLC","11.5*13-BGA153",null,null,"S/T"]
[null,"64G","SDINBDA4-64G","v5.1","3D TLC","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","SDINBDG4-16G-XA","v5.1","MLC","11.5*13-BGA153","A3","-40 ~ +85","S/T"]
[null,"16G","SDINBDA6-16G","v5.0","3D TLC","11.5*13-BGA153",null,"-25 ~ +85","S/T"]
[null,"32G","SDINBDA6-32G","v5.1","3D TLC","11.5*13-BGA153",null,"-25 ~+85","S/T"]
[null,"16G","SDINBDA2-16G","v5.1","3D TLC","11.5*13-BGA153",null,"-25 ~+85"]
[null,"32G","SDINBDV4-32G","v5.1","96L X3 TLC","11.5*13-BGA153",null,"-25 ~+85"]
[null,"64G","SDINBDV4-64G","v5.1","96L X3 TLC","11.5*13-BGA153",null,"-25 ~+85"]
[null,"128G","SDINBDV4-128G","v5.1","96L X3 TLC","11.5*13-BGA153",null,"-25 ~+85"]
["Micron","4G","3EA28-JW878\n(MTFC4GLWAM-WT)","v4.5",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","3CA28-JW879\n(MTFC8GLWAM-WT)","v4.5",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"4G","1UA18-JW729\n(MTFC4GMTEA-WT)","v4.41",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","2GA28-JW686\n(MTFC8GLSEA-IT)","v4.41",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","3ZA28-JWA48\n(MTFC8GACAAEA-WT)","v4.51","MLC","11.5*13-BGA153",null,"-30 ~ +85","S/T"]
[null,"4G","3ZA28-JWA49\n(MTFC4GACAAEA-WT)","v4.51","MLC","11.5*13-BGA153",null,"-30 ~ +85","S/T"]
[null,"8G","5QA27-JY995\n(MTFC8GAKAJCN-1WMT)","v5.0 ","MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"4G","6FA27-JY976\n(MTFC4GACAJCN-1MWT)","v5.0 ","MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","6FA28-JWB74\n(MTFC16GAKAECN-2MWT)","v5.0 ","MLC","11.5*13-BGA153"]
[null,"32G","5SA28-JWB79\n(MTFC32GAKAECN-3MWT)","v5.0 ","MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"64G","MTFC64GANALAM-WT","v5.1"]
["Toshiba","4G","THGBM5G5A1JBAIR","v4.5","MLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","THGBM5G6A2JBAIR","v4.5","MLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","THGBMAG7A2JBAIR","v4.5","19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"4G","THGBMAG5A1JBAIR","v4.5","MLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","THGBMBG7D4KBAIR","v5.0","A19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"32G","THGBMBG8D4KBAIR","v5.0","MLC/A19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","THGBMBG6D1KBAIL","v5.0","MLC/A19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","THGBMBG7D2KBAIL","v5.0","MLC/A19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","THGBM5G7A2JBAIM","v5.0 ",null,"11.5*13-BGA153"]
[null,"32G","THGBM5G8A4JBAIM","v5.0 ",null,"11.5*13-BGA153",null,null,"S/T"]
[null,"16G","THGBM6G7T2JBAIM","v4.41",null,"11.5*13-BGA153",null,null,"S/T"]
[null,"8G","THGBM6G6T1JBAIR","v4.41",null,"11.5*13-BGA153",null,null,"S/T"]
[null,"16G","THGBM5G7A2JBAIR","v4.5","MLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","THGBMFG7C1LBAIL","v5.0","MLC/15nm","11.5*13-BGA153"]
[null,"4G","THGBMBG5D1KBAIL","v5.0","MLC/A19nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"32G","THGBMFG8C2LBAIL","v5.0","MLC/15nm","11.5*13-BGA153",null,null,"S/T"]
[null,"8G","THGBMFG6C1LBAIL","v5.0","MLC/15nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"4G","THGBMDG5D1LBAIL","v5.1","MLC/15nm","11.5*13-BGA153",null,"-25~+85"]
[null,"8G","THGBMHG6C1LBAIL","v5.1","MLC/15nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"16G","THGBMHG7C1LBAIL","v5.1","MLC/15nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"32G","THGBMHG8C2LBAIL","v5.1","MLC/15nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"64G","THGBMHG9C4LBAIL","v5.1","MLC/15nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"16G","THGBMAG7C2LBAW7","v5.1","MLC/15nm","11.5*13-BGA153","I","-40 ~ +85","S/T"]
[null,"16G","THGBMHG7C2LBAAR","v5.1","MLC/15nm","11.5*13-BGA153","A3","-40 ~ +85","S/T"]
[null,"8G","THGBMHG6C1LBAWL","v5.1","MLC","11.5*13-BGA153","I","-40 ~ +85"]
[null,"16G","THGBMHG7C2LBAW7","v5.1",null,"11.5*13-BGA153","I","-40 ~ +85","S/T"]
[null,"4G","THGBMNG5D1LBAIL","V5.0 ","MLC/15nm","11.5*13-BGA153",null,null,"S/T"]
[null,"8G","THGBMJG6C1LBAU7","V5.1",null,"11.5*13-BGA153","I","-40 ~ +85"]
[null,"8G","THGBMJG6C1LBAIL","V5.1",null,"11.5*13-BGA153",null,"-25~+85"]
[null,"8G","THGBMHG6C1LBAW6","v5.1","MLC","11.5*13-BGA153","I","-40 ~ +85"]
["KIOXIA","16G","THGAMRG7T13BAIL","v5.1",null,"11.5*13-BGA153",null,"-25~+85",null,"eMMC not support 3.3V"]
[null,"32G","THGAMRG8T13BAIL","v5.1",null,"11.5*13-BGA153",{"$nulls":3},"eMMC not support 3.3V"]
[null,"64G","THGAMRG9T23BAIL","v5.1",null,"11.5*13-BGA153",{"$nulls":3},"eMMC not support 3.3V"]
[null,"128G","THGAMRT0T43BAIR","v5.1",null,"11.5*13-BGA153",{"$nulls":3},"eMMC not support 3.3V"]
[null,"64G","THGAMRG9T23BAA8","v5.1",null,"11.5*13-BGA153","A3","-40 ~ +85",null,"eMMC not support 3.3V"]
[null,"4G","THGBMTG5D1LBAIL","v5.0",null,"11.5*13-BGA153","C","-25~+85"]
[null,"64G","THGAMSG9T24BAIL","v5.1","3D TLC/BiCS4","11.5*13-BGA153",{"$nulls":3},"eMMC not support 3.3V"]
["SKhynix","4G","H26M31003GMR","v4.51","MLC/20nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","H26M42003GMR","v4.51","MLC/20nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","H26M52003EQR","v4.51","MLC/20nm","12*16-BGA169",{"$nulls":3},"EOL"]
[null,"8G","H26M41103HPR","v5.0","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"16G","H26M52103FMR","v5.0","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"4G","H26M31001HPR","v4.5","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"32G","H26M64103EMR","v5.0","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"8G","H26M41103HPRL","v5.0","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"8G","H26T43001HPR","v5.0","TLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","H26T55001FPR ","v5.0","TLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"32G","H26T65001EMR","v5.0","TLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","H26M52208FPR","v5.1","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"8G","H26M41204HPR","v5.1","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"32G","H26M64208EMR","v5.1","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"32G","H26M64208EMRA","v5.1",null,"11.5*13*1.0-153FBGA"]
[null,"32G","H26M64208EMRQ","v5.1",null,"11.5*13*1.0-153FBGA"]
[null,"8G","H26M41208HPR","v5.1","MLC/16nm","11.5*13-BGA153",null,null,"S/T"]
[null,"64G","H26M78208CMR","v5.1","MLC/16nm","11.5*13-BGA153",{"$nulls":3},"EOL,LTB：Jun. 30th,\n2019"]
[null,"16G","H26M51002HPR","v5.1","3D V2 MLC","11.5*13-BGA153"]
[null,"32G","H26M62002GMR","v5.1","3D V2 MLC","11.5*13-BGA153"]
[null,"16G","H26M52208FPRI","v5.1","MLC/1ynm","11.5*13-BGA153","I","-40 ~ +85"]
[null,"16G","H26M51002KPR","v5.1",null,"11.5*13*0.8-BGA153",{"$nulls":3},"eMMC not support 3.3V"]
[null,"32G","H26M62002JPR","v5.1",null,"11.5*13*0.8-BGA153",{"$nulls":3},"eMMC not support 3.3V"]
[null,"8G","H26M41208HPRI","v5.1","1ynm/MLC","11.5*13-BGA153","I","-40 ~ +95","S/T"]
[null,"32G","H26M41208EMRA","v5.1","1ynm/MLC","11.5*13-BGA153","A3","-40 ~ +95"]
[]
["Kingston","4G","KE44B26BN","v4.41",null,"12*16-BGA169",{"$nulls":3},"EOL"]
[null,"8G","KE4CV3H5A","v4.41",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","KE4CV4H5A","v4.41",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","KE4CN3K6A","v4.5",null,"12*16-BGA169",{"$nulls":3},"EOL"]
[null,"4G","KE4CN2H5A","v4.5",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","KE4CN4K6A","v4.5",null,"12*16-BGA169",{"$nulls":3},"EOL"]
[null,"16G","EMMC16G-V100","v5.0",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","EMMC08G-V100","v5.0",null,"11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","EMMC08G-M325","v5.1","MLC/15nm","11.5*13-BGA153",null,null,"S/T"]
[null,"8G","EMMC08G-ML36","v5.1"]
[null,"8G","EMMC08G-T227","v5.0","TLC/15nm","11.5*13-BGA153",{"$nulls":3},"Date code greater \nthan 1627 (1st Jul)"]
[null,"32G","EMMC32G-T527","v5.0","TLC/15nm","11.5*13-BGA153",{"$nulls":3},"EOL,Date code greater \nthan 1627 (1st Jul)"]
[null,"16G","EMMC16G-T527","v5.0","TLC/15nm","11.5*13-BGA153",{"$nulls":3},"EOL,Date code greater\n than 1627 (1st Jul)"]
[null,"16G","EMMC16G-M525","v5.1","MLC/15nm","11.5*13-BGA153"]
[null,"4G","EMMC04G-M627","v5.1","MLC/15nm","11.5*13-BGA153",null,"-25~+85",null,"Date code greater \nthan 1627 (1st Jul)"]
[null,"8G","EMMC08G-M728","v5.0","3D MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","EMMC16G-W525","v5.0","MLC/T15nm","11.5*13-BGA153","I","-40 ~ +85","S/T","Industrial"]
[null,"32G","EMMC32G-W525","v5.0","MLC/T15nm","11.5*13-BGA153","I","-40 ~ +85","S/T","Industrial"]
[null,"64G","EMMC64G-W525","v5.0","MLC/T15nm","11.5*13-BGA153","I","-40 ~ +85","S/T","Industrial"]
[null,"16G","EMMC16G-TB28","v5.1","3D TLC","11.5*13-BGA153",null,null,"S/T"]
[null,"4G","EMMC04G-MK27","v5.0",null,"11.5*13-BGA153"]
["FORESEE","32G","NCEFEH58-32G","V4.51","MLC/16nm","11.5*13.5-BGA153",{"$nulls":3},"EOL"]
[null,"8G","NCFSES78-08G","SD 2.0","TLC/21nm","11.5*13.5-BGA153",{"$nulls":3},"EOL"]
[null,"16G","NCEFEH58-16G","V4.51","MLC/16nm","11.5*13.5-BGA153",{"$nulls":3},"EOL"]
[null,"4G","NCEFES88-04G","v4.51","TLC/21nm","11.5*13.5-BGA153",{"$nulls":3},"EOL"]
[null,"8G","NCEFES78-08G","v4.51","TLC/21nm","11.5*13.5-BGA153",{"$nulls":3},"EOL"]
[null,"8G","NCFSESA8-08G","SD 2.0","TLC/19nm","11.5*13.5-BGA153",{"$nulls":3},"fSD, EOL"]
[null,"16G","NCEFBS98-16G","v4.5","TLC/19nm","12*16-BGA169",{"$nulls":3},"注1"]
[null,"4G","NCEFEM48-04G","v4.5","MLC/20nm","11.5*13.5-BGA153"]
[null,"16G","NCEMAH59-16G","v5.0","MLC/16nm","11.5*13-BGA153",null,null,"S/T"]
[null,"32G","NCEMAH59-32G","v5.0","MLC/16nm","11.5*13-BGA153"]
[null,"16G","NCEMBS99-16G","v5.0","TLC/19nm","12*16-BGA169"]
[null,"32G","NCEMBS99-32G","v5.0","TLC/19nm","12*16-BGA169"]
[null,"8G","NCEFAT28-08G","v4.51","TLC/19nm","11.5*13-BGA153",{"$nulls":3},"注1"]
[null,"32G","NCEMBSF9-32G","v5.0 ","TLC/16nm","12*16-BGA169"]
[null,"16G","NCEMBSF9-16G","v5.0 ","TLC/16nm","12*16-BGA169"]
[null,"8G","NCEMASD9-08G","v5.0","TLC/16nm","11.5*13-BGA153",{"$nulls":3},"仅支持PRV版本4.3及之后版本"]
[null,"16G","NCEMBD39-16G","v5.0","MLC/15nm","12*16-BGA169"]
[null,"16G","NCEMAD6B-16G","v5.1","TLC/15nm","11.5*13-BGA153"]
[null,"8G","NCEMAD7B-08G","v5.0 ","TLC/15nm","11.5*13-BGA153"]
[null,"8G","NCEMAM6G-08G","v5.1","MLC/16nm","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","NCEMASKG-16G","v5.1","TLC/14nm","11.5*13-BGA153",null,null,"S/T"]
[null,"32G","FSEWASLG-32G","v5.1",null,"11.5*13-BGA153","I","-40 ~ +85"]
[null,"16G","NCEMAD99-16G","v5.0 ",null,"11.5*13-BGA153"]
[null,"32G","NCEMASLD-32G","v5.1",null,"11.5*13.5-BGA153","C","-25 ~ +85"]
[null,"16G","NCEMAD9D-16G","v5.1",null,"11.5*13.5-BGA153"]
[null,"32G","FSEIASLD-32G","v5.1",null,"11.5*13.5-BGA153",null,"-25~+85"]
[null,"8G","NCEMAD9D-8G","v5.1",null,"11.5*13.5-BGA153"]
[null,"8G","FEMDNN008G-08A39","v5.1",null,"FBGA 11.5*13.5*1.0",null,"-25~+85"]
[null,"8G","FEMDRM008G-58A39","v5.1",{"$nulls":3},"-25~+85"]
[null,"16G","FEMDNN016G-58A43","v5.1",null,"FBGA 11.5*13.5*1.0",null,"-25~+85"]
[null,"4G","FEMDNN004G-58A42","v5.1",null,"FBGA 11.5*13.5*0.8",null,"-25~+85"]
[null,"32G","FEMDNN032G-58A46","v5.1",null,"FBGA 11.5*13.5*1.0",null,"-25~+85"]
[null,"32G","FEMDRM032G-A3A55","v5.1",null,"FBGA 11.5*13.5*1.0",null,"-25~+85"]
[null,"128G","FEMDNN128G-A3A44","v5.1",null,"FBGA 11.5*13.5*1.0",null,"-25~+85"]
["AcSip","8G","NCMMCS08G","v4.5",null,"12*16-BGA169"]
[null,"16G","NCMMCS16G ","v4.5",null,"12*16-BGA169"]
["AVEXIR","16G","AVEC016G-FA6","v4.5",null,"11.5*13-BGA153",null,null,"S/T"]
["EUDAR","8G","EMS1ASCBT1FC008","v4.51",null,"11.5*13-BGA153"]
[null,"16G","EMS1ASCBT2FC016","v4.51",null,"11.5*13-BGA153"]
[null,"16G","EMB1CTTD41FC016","v5.1",null,"11.5*13-BGA153"]
[null,"32G","EMB1CTTD51FC032","v5.1",null,"11.5*13-BGA153"]
["Barun","4G","BEM04M5B50XA-A3CT","v4.51","MLC/20nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"4G","BEM04S2B60XA-A3CT","v4.51","TLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"8G","BEM08S1B60XA-A3CT","v4.51","TLC/19nm","11.5*13-BGA153",{"$nulls":3},"EOL"]
[null,"16G","BSB16GCDRS4EM-01","v4.51","TLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"8G","BSA08GCDRS4EM-01","v4.51","TLC/16nm","11.5*13-BGA153",null,"-25~+85","S/T"]
[null,"16G","BTA16GCFHAEET","v5.1","TLC/15nm","11.5*13-BGA153"]
["Ramaxel","16G","REMKDM316GDBB","v5.0","MLC","11.5*13-BGA153"]
[null,"8G","REMKDM308GSBB","v5.0","MLC","11.5*13-BGA153"]
[null,"16G","REMSAT416GDBB","v5.0","TLC/A19nm","11.5*13-BGA153",null,null,"S/T"]
[null,"8G","REMSAT408GSBB","v5.0","TLC/A19nm","11.5*13-BGA153"]
[null,"8G","REMPBT808GSBB","v5.0","TLC/15nm","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","REMPBT716GSBB","v5.0","TLC/15nm","11.5*13-BGA153",null,null,"S/T"]
["Spansion/\nSkyHigh","8G","40410081B1B1W00","v4.51","MLC","11.5*13-BGA153",null,"-25~+85",null,"EOL,LTB:2016-10-5"]
[null,"16G","40410161B1B1W01","v4.51","MLC","11.5*13-BGA153",null,"-25~+85",null,"EOL,LTB:2016-10-5"]
["Gigadevice","8G","GD9E8MUYNM-MA00","v5.0 ","MLC","11.5*13-BGA153"]
[null,"8G","GD9E8M00YNI","v5.0 ","MLC","11.5*13-BGA153"]
[null,"4G","GD9E4M00YNI","v5.0 ","MLC","11.5*13-BGA153"]
[null,"8G","GD9E8T00GNM-05","v5.1","TLC/T16nm","11.5*13-BGA153"]
["FDI","4G","MC1M04M1L3AB","v4.51","MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"8G","MC1M08M2L3AB","v4.51","MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","MC1M16M4L3AB","v4.51","MLC","11.5*13-BGA153",null,null,"S/T"]
["SiS","8G","TC008000AA","v5.0","TLC/S16nm","11.5*13-BGA153",{"$nulls":3},"Don't support when EXT_CSD[261:254]=0x44010000000"]
[null,"8G","MC008000AA","v5.0","MLC/H16nm","11.5*13-BGA153"]
[null,"16G","MC016000AA","v5.0","MLC/H16nm","11.5*13-BGA153"]
[null,"32G","MC032000AA","v5.0","MLC/H16nm","11.5*13-BGA153"]
["Dosilicon","16G","FMR16C1D0A-SB","v5.0","H3D V2 MLC","11.5*13-BGA153",null,null,"S/T"]
["JSC","32G","JSMC32BUA2HYAEA","v5.0","H3D V2 MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"16G","JSMC16AUA2HYAEA","v5.0","H3D V2 MLC","11.5*13-BGA153",null,null,"S/T"]
[null,"8G","JSMC08AUM1ASAEA-H5","v5.1",null,"11.5*13-BGA153"]
["ESSENCORE","16G","ENEAGQ8BE1MR-HB","v5.1",{"$nulls":3},"-20 ~ +60"]
[null,"8G","I3E-8GTH7CMRE","v5.0","MLC/T16nm","11.5*13-BGA153"]
["EOREX ","32G","EMMF5BA-032G","v5.1",null,"11.5*13-BGA153"]
["Biwin","4G","BWCMARD11G04G","v5.0",{"$nulls":3},"-25 ~ +85"]
[null,"8G","BWCTASC11G08G","V5.0",null,"9*11-BGA153"]
[null,"8G","BWCMMQ511G08G","V5.0",null,"11.5*13-BGA153"]
[null,"16G","BWCTAK611G16G","V5.0",null,"11.5*13-BGA153"]
[null,"64G","BWCTARV11X64G","V5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
[null,"8G","BWCE28NH-08G","V5.0",null,"11.5*13*0.9"]
["MXIC","8G","MX52LM08A11XVI","V5.1","MLC","11.5*13-BGA153","I","-40 ~ +85"]
["TOPDISK","16G","A121-16G","V5.1",null,"11.5*13-BGA153"]
[null,"32G","A132-32G","V5.1",null,"11.5*13-BGA153"]
["UniIC","32G","UNMEN05GC1C31AS","v5.1","3D TLC","11.5*13-BGA153","C","-25 ~ +85","S/T"]
[null,"64G","UNMEN06GC2C31AS","v5.1","3D TLC","11.5*13-BGA153","C","-25 ~ +85"]
["Artmem","8G","AT70B08GT05C","v5.1","2D TLC/15nm","11.5*13-BGA153",{"$nulls":3},"非工业"]
[null,"16G","AT70B16G4T02C","v5.1","3D TLC/Bics3","11.5*13-BGA153",{"$nulls":3},"非工业"]
[null,"16G","AT70B16G4T05C","v5.1","3D TLC/Bics3","11.5*13-BGA153",{"$nulls":3},"非工业"]
[null,"32G","AT70B32GT01C","v5.1","3D TLC/Bics3","11.5*13-BGA153",{"$nulls":3},"非工业"]
[null,"64G","AT70B64GT01C","v5.1","3D TLC/Bics3","11.5*13-BGA153",{"$nulls":3},"非工业"]
[null,"16G","AT70B16G3S02C","v5.1","2D MLC/K9GDGD8U0B","11.5*13-BGA153",{"$nulls":3},"非工业"]
[null,"16G","AT70B16G3S06F","v5.1",null,"11.5*13-BGA153"]
[null,"32G","AT70B32G3S01C","v5.1","3D TLC/K9AFGD8H0A","11.5*13-BGA153",{"$nulls":3},"非工业"]
[null,"8G","AT70B08G3Y02F","v5.1",null,"11.5x13x0.92",null,"-40 ~ +85"]
[null,"8G","AT70B08G3Y02F2","v5.1",{"$nulls":3},"-40 ~ +85"]
[null,"16G","AT70B16G3Y02F","v5.1",null,"11.5x13x0.92",null,"-40 ~ +85"]
[null,"8G","AT70B08G3S03F","v5.1","MLC","11.5*13-BGA153"]
[null,"16G","AT70B16G4T06F","v5.1",null,"11.5*13-BGA153"]
[null,"16G","AT70B16GS10F","v5.1"]
[null,"16G","AT70B16G4S10F","v5.1"]
[null,"8G","AT70B8GY02F","v5.1"]
[null,"32G","AT70B32G4Y01F","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
[null,"64G","AT70B64G4Y01F","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
["ISOCOM","32G","MEMA032G-M0S00","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
["SCY","4GB","E04GDML31ABE00","v5.1",{"$nulls":3},"-25 ~ +85"]
[null,"32G","E32GDDF11ABE00","v5.1","TLC ","11.5*13-BGA153",null,"-25 ~ +85"]
["YMTC","32G","YMEC6A2TB1A2C3","v5.1","MLC","11.5*13-BGA153",null,"-25 ~ +85"]
[null,"64G","YMEC7A2TB2A2C3","v5.1","MLC","11.5*13-BGA153",null,"-25 ~ +85"]
[null,"64G","YMEC7B0TE1A2C3","v5.1","3D TLC","11.5*13-BGA153",null,"-25 ~ +85"]
[null,"128G","YMEC8B0TE2A2C3","v5.1","3D TLC","11.5*13-BGA153",null,"-25 ~ +85"]
["SkyHigh","4G","S40FC004C1B1C","v5.1","MLC","11.5*13-BGA153","I","-40 ~ +85"]
["Konka Kowin","8G","KAS03111","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
[null,"16G","KASG5111","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
["SiliconGo","32G ","SGM8100C-Y02BBG","v5.1",null,"11.5*13-BGA153",null,"-40 ~ +85"]
[null,"16G","SGM8000C-S21BAG","v5.1",null,"11.5*13-BGA153","I","-40 ~ +85"]
["Core\nStorage","8G","CME4A0TD-08GA","v5.1","pMLC","FBGA153\n11.5 x 13 x 1.0",null,"-40 ~ +85"]
["Metorage","32G ","MIE3032CH7","v5.1",null,"BGA153",null,"-25 ~ +85"]
[null,"64G ","MIE3064CH7","v5.1",null,"BGA153",null,"-25 ~ +85"]
[null,"8G","MPE3008EH7","v5.1","pSLC","BGA153",null,"-40 ~ +85"]
[null,"16G","MPE3016EH7","v5.1","pSLC","BGA153",null,"-25 ~ +85"]
["GOKE","8G","XPA72EA0E-008","v5.1","MLC ","11.5*13-BGA153",null,"-25 ~ +85"]
[null,"32G ","XPB73EA0E-032","v5.1","TLC","11.5*13-BGA153",null,"-25 ~ +85"]
["HIKSEMI","16G","HSEMSES2S2B16G","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
[null,"32G ","HSEMSDS6S2B32G","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
["NanoWell","64G","NW-EM064G","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
[null,"128G ","NW-EM128G","v5.1",null,"11.5*13-BGA153",null,"-25 ~ +85"]
["HKCS","16G","D016C1YJCD-E00","v5.1",{"$nulls":3},"-25 ~ +85"]
[null,"32G","D032C1YJCD-E00","v5.1",{"$nulls":3},"-25 ~ +85"]
[]
["注1：支持该eMMC需要将各环节MMC驱动更新到最新，并修改sys_config.fex让该eMMC工作在SDR模式下。"]

{"sheet":"5-声明","index":4,"n_rows":6,"n_cols":1,"rows_kept":6,"merged":[[2,0,2,17],[3,0,3,20],[5,0,5,20]],"flags":["formulas_cached_only"]}
[]
[]
["• Declaration"]
["This document is the original work and copyrighted property of Allwinner Technology (“Allwinner”). Reproduction in whole or in part must obtain the written approval of Allwinner and give clear acknowledgement to the copyright owner."]
[]
["The information furnished by Allwinner is believed to be accurate and reliable. Allwinner reserves the right to make changes in circuit design and/or specifications at any time without notice. Allwinner does not assume any responsibility and liability for its use. Nor for any infringements of patents or other rights of the third parties which may result from its use. No license is granted by implication or otherwise under any patent or patent rights of Allwinner. This datasheet neither states nor implies warranty of any kind, including fitness for any particular application. "]